Home / Services / Gym Fitouts
Gym & Fitness Fitouts

# Gym & fitness centre fitouts built for heavy loads

We build gym and fitness centre fitouts for independent operators, franchise brands and corporate wellness centres across Brisbane and the Gold Coast — commercial gyms, boutique studios, PT facilities and health clubs that are structurally sound for heavy equipment loads, operationally efficient and code-compliant.

Get a fixed-price proposal
See our projects
What a gym fitout involves

## Structural requirements that set gyms apart

Structural reinforcement of floors for free-weight zones, vibration isolation for cardio equipment, rubber flooring systems capable of withstanding impact and equipment loads, and adequate ceiling height for functional training rigs are all early design considerations.

Change rooms with shower and locker facilities require commercial-grade waterproofing, ventilation and disability access. We manage all of these elements as part of the fitout scope.

Fitness spaces we build

## Every zone of a modern facility

### Gym floor — cardio & resistance

Rubber flooring systems appropriate to equipment and traffic, slab-level provisions for anchoring racks and rigs, and services provisions for cardio equipment electrical connections.

### Free weights & functional zones

Reinforced flooring to absorb dropped-weight impact, ceiling clearance for overhead movements, and structural provisions for wall-mounted rigs, suspension anchors and cable machines.

### Group fitness rooms

Sprung or acoustic floor systems, mirror walls, dimmable or high-intensity lighting, sound system rough-in and ventilation calculated for exercise-intensity occupancy.

### Change rooms & amenities

Heavy-duty commercial waterproofing in showers, non-slip flooring, structural provisions for bolted locker banks, bench seating, vanities and accessible facilities to AS 1428.

### Reception & retail

Reception counters with integrated POS and access control, retail display shelving for supplements and apparel, and feature wall treatments that establish the member experience.

Compliance

## Flooring for gyms

Flooring is one of the most critical and specialised elements of a gym fitout. We supply and install the full range to suit each zone and equipment type.

- Rolled rubber — heavy-duty 8–15mm for free-weight zones
- Interlocking rubber tiles — functional zones & group fitness
- Vinyl — reception, change rooms & yoga studios
- Sprung timber or floating systems — dance & martial arts
- Structural anchor provisions for rigs & cable machines
- Change-of-use approvals managed where required

Gym Fitouts FAQ

## Questions we're often asked

Yes. We design and install structural anchor provisions for wall-mounted and floor-mounted equipment. For heavy functional training rigs, we assess the existing slab capacity and provide additional structural support where required.
Most gym fitouts within an existing commercial tenancy require a building approval. Change-of-use approvals may also be needed if the premises was previously a different use class. We manage these approvals.
A boutique studio (100–200 sqm) typically takes 6–10 weeks. A full commercial gym (500–1000 sqm) may take 12–18 weeks. Timeline is driven by the extent of change room and wet area works.
Yes. We build from franchise design packages and understand the design control processes of fitness franchise operators.
Let's talk

## Plan your gym or fitness fitout in Brisbane or the Gold Coast

Call us or send your brief — we'll arrange a no-obligation site inspection and a detailed fixed-price proposal.

Request a proposal
Call 0488 773 232