Asbestos Roof Removal

# Asbestos Roof Removal

Licensed removal of asbestos cement roofing across Brisbane, Gold Coast and SEQ. Super-six corrugated and flat fibro roofing are among the most common asbestos materials on Queensland homes built before 1990 — and become more dangerous as they age.

Request a Free Quote
Emergency 0488 773 232
Overview

## Ageing roof sheeting is an increasing risk

As asbestos cement roofing ages it degrades, becomes brittle and friable, and poses an increasing risk to occupants and neighbouring properties. Roofing in poor condition — cracked, broken, heavily weathered or lichen-covered — must be treated with particular care.

Asbestos roof removal over 10m² requires a licensed removalist. We hold an A-Class licence, covering all categories of asbestos roof sheeting in any quantity and condition. We use wet suppression throughout and never dry-cut or break sheets unnecessarily.

What we remove

## All asbestos roofing types

### Corrugated & flat sheeting

Super-six corrugated asbestos cement sheeting and flat asbestos cement sheet roofing, removed intact where possible.

### Ridge capping & flashing

Asbestos cement ridge capping, flashings and roofing underlay or sarking.

### Ready for re-roofing

Once removed, your property is ready for Colorbond, terracotta, concrete tile or membrane roofing — we can coordinate with roofers.

Our process

## Controlled removal, start to finish

- #### Inspection & quote

  We inspect the roof, assess condition and extent of ACM, and provide a fixed-price quote including disposal.

- #### WHSQ notification

  We notify WHSQ at least five business days prior to commencing where required.

- #### Access & safety setup

  Fall protection, scaffolding or roof access equipment is erected. The ground below is protected and access restricted.

- #### Controlled removal

  Sheets are removed carefully and intact where possible, with wet suppression used throughout. All debris is collected and bagged.

- #### Bagging & transport

  All ACM is double-wrapped or containerised, labelled, and transported under a hazardous-waste manifest to a licensed facility.

- #### Site clean & clearance

  The surrounding area is cleaned and documentation provided, including waste disposal receipts.

Common questions

## Asbestos roof removal questions

No. Removal of more than 10m² of asbestos cement roofing requires a licensed removalist in Queensland. Even smaller areas require careful handling and licensed disposal of the waste.

Costs depend on the roof area, accessibility, pitch, condition of the sheeting and disposal weight. We provide fixed-price itemised quotes — contact us for a quote specific to your property.

For non-friable sheeting in good condition, temporary exclusion from the immediate work area is typically sufficient. For deteriorated or friable sheeting we may recommend temporarily vacating. We advise at the quotation stage.

Yes. Licensed disposal is included in our quote. We transport all asbestos waste to an EPA-approved facility and provide waste disposal documentation.

Related services

## Manage the whole project under one licence

Because we hold both an A-Class Asbestos Removal Licence and a Queensland Demolition Licence, we can carry the related work below under the same contract.

Asbestos Removal & Disposal Emergency Asbestos Clean Up Asbestos Testing Residential Demolition
Free, no-obligation quote

## Get a free asbestos roof removal quote

Safe, licensed removal with disposal included — and a clear path to re-roofing across Brisbane, Gold Coast and SEQ.

Request a Free Quote
Call 0488 773 232