Roof Ventilation

# Roof ventilation systems — Brisbane and Gold Coast

A well-ventilated roof cavity is one of the most effective, underrated improvements you can make to a Queensland home — cutting heat, moisture and cooling costs.

Get a free quote
Call 0488 773 232

## An unventilated roof is a heat trap

Without adequate ventilation, the roof space becomes a heat trap — reaching 60°C or more on a Brisbane summer afternoon — and a moisture accumulator that accelerates timber decay, encourages mould and forces air conditioning to work harder. Innovare Roofing designs and installs ventilation systems for residential and commercial properties across SEQ.

Effective ventilation reduces peak roof cavity temperature by 15–25°C, directly reducing cooling energy consumption and extending the life of insulation, sarking and structural timbers.

Products We Install

## Passive and powered ventilation

### Whirlybirds

Wind-driven turbine ventilators — the most common residential product in SEQ. Quiet, durable and effective in sea-breeze conditions when correctly positioned.

### Ridge Vents

Continuous vents along the ridge line release hot air from the highest point while drawing cool air through eave vents — more discreet than whirlybirds.

### Powered Ventilators

Electrically powered fans that draw air regardless of wind — ideal for low-wind urban sites or complex roof geometries.

### Solar Ventilators

Solar-powered extraction — no household wiring, maximum performance on the hottest, sunniest part of the day. Highly practical for Queensland.

Balanced Design

## Extraction and intake must be balanced

Installing whirlybirds or ridge vents without adequate eave or soffit intake simply creates resistance — the ventilators underperform. We assess the full system.

- Intake at the eaves — soffit venting to feed cool air in.
- Extraction at the ridge — where heat accumulates most intensely.
- Correct quantity & placement — roughly one whirlybird per 50 m² of roof space.
- Retrofit-ready — ridge vents fitted to existing corrugated and ribbed metal roofs.
- Sarking synergy — ventilation flushes hot air so reflective sarking performs better.
- Whole-of-home comfort — reduced ceiling heat load and lower cooling costs.

Common Questions

## Frequently asked questions

A rough guide is one whirlybird per 50 m² of roof space for standard residential use. Roof geometry, pitch, insulation and local wind patterns all affect the optimal number — we assess each home individually.

In Queensland’s high-sunshine environment, solar-powered ventilators provide excellent value. They operate most powerfully on the hottest days when ventilation is most needed, and require no electrical installation.

Yes. Ridge vent systems are available for retrofit on existing corrugated and ribbed metal roofing profiles. We cut the existing ridge, install the vent and apply compatible flashings.

In most cases, yes. Reducing peak roof cavity temperatures reduces the heat load on ceilings, which reduces the work your air conditioning does. Savings depend on your insulation level, house size and usage patterns.

Related Services

## Explore more roofing services

Fascia & Soffit
Skylights
Metal Roofing
Domestic Roofing
Free, No-Obligation Quote

## Improve your home’s comfort and efficiency

Book a roof ventilation assessment and we’ll design a balanced system for your home.

Request a quote
Call 0488 773 232