Remedial service

# Asbestos Encapsulation, Brisbane & Queensland

Application of a penetrating or bridging encapsulant to asbestos-containing materials in sound condition — a recognised, regulated management option under Queensland WHS legislation where removal is not required or appropriate.

Request a Consultation
Call 0488 773 232
When it applies

## Managing asbestos in place, safely and lawfully

Asbestos encapsulation is the application of an encapsulant to asbestos-containing materials (ACMs) that are in sound condition and are not suitable for, or do not require, immediate removal. It is a recognised and regulated management option under the Queensland Work Health and Safety Regulation 2011 and the relevant Code of Practice.

We apply encapsulation where removal would introduce greater disturbance risk than in-situ management — common in heritage buildings, occupied residential properties, and where the ACM is in good condition and inaccessible.

### When encapsulation is appropriate

The ACM (typically non-friable asbestos cement — fibro cladding, eave linings, floor tiles) is in sound condition; removal would require major structural disturbance not otherwise warranted; the property is being retained; an asbestos management plan specifies encapsulation; or budget or heritage constraints make removal impractical at the time. It is not appropriate for friable asbestos, deteriorated ACMs, or materials that will be disturbed by subsequent works.

Our process

## Our compliant process

1. #### Survey & management plan

   We require an asbestos survey and, ideally, a current asbestos management plan before commencing — and can arrange an accredited assessor survey if one is not in place.

2. #### Licensed engagement

   For class A or class B licensed asbestos work, we engage appropriately licensed asbestos contractors and coordinate the works.

3. #### Clearance inspection

   Encapsulation is preceded by a clearance inspection from an accredited asbestos assessor.

4. #### Encapsulation

   Quality encapsulant products are applied to sound ACM in accordance with Queensland WHS legislation and the relevant Codes of Practice.

5. #### Documentation

   Works are recorded in the property’s asbestos register and management plan, with a post-works report and recommended re-inspection intervals.

Regulated & documented

## A compliant management option

Quality encapsulant products, properly applied to sound ACM, typically provide protection for 10–20 years, subject to re-inspection. All work is carried out under Queensland WHS legislation.

- Compliant with the QLD WHS Regulation 2011
- Accredited assessor clearance inspection
- Licensed class A/B contractors engaged where required
- Recorded in the asbestos register and management plan
- Post-works report with re-inspection intervals
- Integrated with broader remedial and restoration scopes

Asbestos Encapsulation — FAQs

## Common questions

Non-friable asbestos cement in good condition, where fibres are bound within the cement matrix and the surface is not disturbed, presents a very low risk. Risk increases significantly if the material is drilled, sanded, cut or otherwise disturbed. Encapsulation provides an additional surface seal to reduce fibre release from minor contact or weathering.

Where removal is the appropriate option, we work with licensed asbestos removal contractors and coordinate removal as part of a broader scope. We do not carry out class A or class B removal directly but manage the process on behalf of our clients.

Yes. We require an asbestos survey and, ideally, a current asbestos management plan for the property before commencing. We can arrange an accredited asbestos assessor survey if one is not in place.

Quality encapsulant products, properly applied to sound ACM, typically provide protection for 10–20 years, subject to re-inspection. We provide a post-works report and recommended re-inspection intervals.

Related services

## You may also need

Defect Rectification
Heritage Restoration
Remedial Consultation
Get started

## Managing asbestos in your building?

We coordinate compliant, documented in-situ management. Request a consultation to discuss the right approach for your property.

Request a Consultation
Call 0488 773 232