Home / Services / Medical Fitouts
Medical Centre Fitouts

# Medical centre fitouts built to clinical & compliance standards

We design and construct medical centre fitouts across Brisbane — including the CBD, Spring Hill, Chermside, Aspley and Eight Mile Plains — and the Gold Coast. GP clinics, allied health practices, specialist suites and bulk-billing centres that meet Queensland Health guidelines, the NCC and AS 1428 access requirements.

Get a fixed-price proposal
See our projects
What makes a medical fitout different?

## Compliance obligations general fitouts don’t carry

Infection control requirements influence materials selection — impervious wall surfaces, coved skirting, seamless flooring, and handwashing facilities positioned to clinical flow. Queensland Health infrastructure guidelines specify minimum room dimensions, ventilation rates and bathroom ratios. Privacy Act requirements drive the acoustic treatment of consulting rooms, and AS 1428 governs door widths, hardware, accessible consulting rooms and reception counter heights.

Builders without healthcare experience regularly underestimate these requirements. We have delivered multiple healthcare tenancy fitouts and understand both the compliance framework and the operational reality of clinical settings.

Medical spaces we build

## For every model of care

### General practice clinics

Waiting areas with infection-resistant finishes, accessible reception counters, consulting rooms with handwash basins and exam lighting, treatment rooms, sterilisation, medication storage and accessible bathrooms — designed for efficient patient flow.

### Allied health practices

Physiotherapy, OT, psychology, podiatry and speech pathology — each with sector-specific needs, from clear treatment floor area to high acoustic performance between consulting rooms.

### Specialist consulting suites

Higher-specification finishes, specialist procedure room infrastructure (medical gas, imaging support), and premium waiting environments appropriate to the specialist’s patient demographic.

### Bulk billing & community health

Efficient patient flow, robust finishes that withstand heavy daily use, and layouts accommodating multiple practitioners with shared support functions.

Compliance

## The medical compliance framework

We coordinate structural and services work while your architect drives the clinical design — guiding you through the relevant approval pathway, including any Queensland Health review for licensed health services.

- NCC BCA Class 9a health care provisions (where applicable)
- Queensland Health guidelines for non-government health infrastructure
- AS 1428 access — all patient-facing areas
- Infection control & hand hygiene per NHMRC guidelines
- Medical gas AS 2896 (where provisions are included)
- Fire safety — sprinkler, fire doors, emergency lighting, exit signage

Materials & finishes for healthcare

## Specified for infection control

Every surface in a clinical setting is chosen for cleanability, durability and compliance — from coved skirtings to antibacterial joinery.

Flooring
Homogenous vinyl (Tarkett, Forbo), epoxy resin or polished concrete with coved skirtings
Walls
Moisture-resistant plasterboard, vinyl wall cladding, or porcelain tile in wet & treatment areas
Joinery
Laminate-faced cabinetry with antibacterial surfaces, integrated basin units
Ceilings
Vinyl-faced tiles in clinical areas, plasterboard with access panels for services
Doors
Solid-core acoustic-rated doors, lever handles to AS 1428, vision panels in treatment areas
Medical Fitouts FAQ

## Questions we're often asked

Yes. We work collaboratively with healthcare architects, practice managers and equipment suppliers. We manage structural and services coordination while the architect drives the clinical design.
Most medical fitouts require a building approval from a private certifier or council. If the facility is a licensed health service, additional Queensland Health review may be required. We guide clients through the relevant pathway.
A mid-size GP clinic of 200–350 sqm typically takes 8–14 weeks from approval. Larger multi-practitioner centres can take 16–22 weeks depending on scope.
Yes. We coordinate with equipment suppliers (examination couches, sterilisation units, imaging, medical gas outlets) to ensure rough-in provisions are correct prior to finishes installation.
Let's talk

## Plan your medical centre fitout in Brisbane or the Gold Coast

Call us or send your brief — we'll arrange a no-obligation site inspection and a detailed fixed-price proposal.

Request a proposal
Call 0488 773 232