Home / Services / Childcare Fitouts
Childcare Centre Fitouts

# Safe, compliant childcare centres designed for learning

We build childcare centre fitouts across Brisbane and the Gold Coast for operators who need a construction partner who understands the National Quality Framework, the Education and Care Services National Regulations, and the physical environment requirements of early childhood education.

Get a fixed-price proposal
See our projects
The regulatory framework

## Commercial building, child safety & education regulation

The Education and Care Services National Regulations (under the NQF) specify minimum indoor and outdoor space per child, fencing and gate requirements, kitchen and hygiene facilities, and service environment requirements. The Regulatory Authority (Queensland Department of Education) assesses the physical premises against the NQF, and the NCC governs building safety, access and services.

Any builder operating in this sector without a working understanding of all three frameworks creates risk for the operator. We build to all three.

Childcare spaces we build

## Indoor and outdoor environments

### Indoor learning rooms

Sized to the NQF indoor space per child (typically 3.25 sqm), with cushioned vinyl or carpet flooring, integrated washing and nappy facilities, child-height storage and natural lighting.

### Outdoor play areas

Compliant fencing (min 1.2m, self-closing self-latching gates), certified softfall to AS 4422 and AS 4685 under play equipment, shade structures and compliant drainage.

### Kitchens & laundries

Food-safe kitchen (FSANZ) sized to the service’s meal programme, plus laundry facilities for nappy and linen management to NQF guidelines.

### Nappy change & bathrooms

Nappy change benches, handwashing at child and adult heights, child-sized toilets, and visible change areas in line with safeguarding requirements.

### Sleep rooms

Appropriate ventilation, acoustic separation from active play areas, and space for portable cots or sleeping mats to NQF per-child requirements.

### Administration & staff areas

Office, staff room and resource storage for management and educators, meeting NQF and reasonable staff amenity standards.

Compliance

## Safety standards for childcare builds

Childcare centres are Class 9b buildings under the NCC requiring building development approval. We manage the approval process, including coordination with the Regulatory Authority where required.

- Education and Care Services National Regulations 2011
- National Quality Standards — Quality Area 3: Physical Environment
- AS 4422 — Playground surfacing
- AS 4685 — Playground equipment
- NCC BCA for building safety, fire and access
- AS 1428 for disability access across the premises

Childcare Fitouts FAQ

## Questions we're often asked

Yes. Childcare centres are Class 9b buildings under the NCC, requiring building development approval. We manage the approval process including coordination with the Regulatory Authority where required.
Yes. Childcare centres in mixed-use buildings, shopping centres and office towers are increasingly common. We manage the interface with base-building systems and centre management approval processes.
The NQF requires premises to be enclosed so children cannot leave without adult accompaniment. Specific fencing heights and gate hardware are specified in the Regulations. We build compliant perimeter fencing and gate systems.
We prepare structural and surface provisions for playground equipment and coordinate with the supplier on installation sequencing. Final certification of the play equipment is provided by the supplier.
Let's talk

## Plan your childcare centre fitout across Brisbane & Gold Coast

Call us or send your brief — we'll arrange a no-obligation site inspection and a detailed fixed-price proposal.

Request a proposal
Call 0488 773 232