24/7 emergency service

# Fire Damage Restoration Brisbane & Gold Coast

The structured, documented process of fire damage restoration Brisbane — making a fire-affected building safe, removing damaged material, remediating smoke and soot, and reinstating it to a safe, code-compliant condition — while working closely with insurers and loss adjusters.

24/7 Emergency · 0488 773 232 Request a Consultation
Emergency response · Brisbane & Gold Coast

### Fire service cleared the site? Secure the building next.

Immediate make-safe protects the structure from weather and unauthorised access. We mobilise across Brisbane and the Gold Coast as soon as access is permitted.

Call 0488 773 232
After a Fire

## Thorough, Well-documented Restoration

Fire damage restoration is the structured process of providing Fire Damage restoration Brisbane, making a fire-affected building safe, removing fire-damaged material, remediating smoke and soot contamination, and reinstating the building to a safe, code-compliant condition.

Innovare Remedial responds to fire damage events across Brisbane and South East Queensland, working closely with insurers, loss adjusters and fire investigators. Smoke and soot contamination penetrates porous surfaces well beyond the directly fire-affected zone — so thorough remediation is essential for indoor air quality and to prevent ongoing odour and surface contamination.

Our Process

## The Restoration Process After A Fire

1. #### Emergency make-safe

   Following clearance from the fire service and insurer, we erect hoardings or temporary enclosures, board openings, install temporary roofing and establish safe exclusion zones — protecting the structure and preventing unauthorised access.

2. #### Structural assessment

   A thorough condition survey identifies elements compromised by fire, heat, smoke or firefighting water. A structural engineer is engaged where required to assess load-bearing elements and specify repair or demolition.

3. #### Strip-out & waste removal

   All non-salvageable material is removed under a controlled scope — charred framing, damaged plasterboard, fire-affected insulation and contaminated fixtures — with asbestos screening on older properties before disturbance.

4. #### Smoke, soot & odour remediation

   Affected surfaces are cleaned and treated with HEPA vacuuming, chemical sponge wipe-down, and thermal fogging or ozone treatment to eliminate odour from cavities and surfaces.

5. #### Reinstatement

   All elements are reinstated to NCC/BCA standards, with full photographic documentation and building-certifier inspection at key stages where required.

6. #### Insurance coordination

   We provide itemised scope-of-works, structural engineering reports, progress photos and completion documentation to support the claim through to finalisation.

Beyond the burn zone

## Structure, air quality and odour — all addressed

Minor fire events with localised damage can be remediated in 2–4 weeks. Major structural fires requiring significant rebuild can take 3–9 months. We provide a programme at the scoping stage and maintain regular communication.

- Rapid make-safe once access is permitted
- Structural engineer assessment of load-bearing elements
- Asbestos screening before strip-out on older buildings
- HEPA, chemical and thermal/ozone smoke & odour treatment
- NCC/BCA-compliant reinstatement with certifier inspection
- End-to-end insurer and loss-adjuster coordination

Fire Damage Restoration — FAQs

## Common Questions

Not until it has been declared safe by the fire service and, where applicable, a structural engineer. Structural instability and atmospheric hazards (carbon monoxide, particulates) make fire-affected buildings extremely dangerous immediately after an event. Call us for emergency make-safe as soon as access is permitted.

Yes. Smoke travels throughout a building during and after a fire, depositing soot and volatile organic compounds on surfaces well beyond the fire’s origin. Thorough smoke and soot remediation is essential for indoor air quality and to prevent ongoing odour and surface contamination.

Fire events are one of the most common triggers for major loss claims. We work directly with your insurer and loss adjuster from the first call, providing the scope, assessment reports and progress documentation they require. See Insurance Repair Works.

Minor fire events with localised damage can be remediated in 2–4 weeks. Major structural fires requiring significant rebuild can take 3–9 months. We provide a programme at the scoping stage and maintain regular communication throughout.

Related services

## You may also need

Storm Damage
Structural Repair
Insurance Repair Works
Get started

## Recovering from a fire?

We handle the building so you can focus on everything else. Call our emergency line or request a consultation to begin a documented rebuild.

Request a Consultation
Call 0488 773 232