Metal Roofing

# Metal roofing specialists — Brisbane and Gold Coast

Colorbond, Zincalume and architectural metal roofing — profiles and fastening patterns specified for SEQ’s demanding wind and weather environment, by a BlueScope-accredited installer.

Get a free quote
Call 0488 773 232

## The dominant roofing system in SEQ — for good reason

Innovare Roofing installs Colorbond steel, Zincalume and architectural metal roofing across Brisbane, the Gold Coast and South East Queensland. As a BlueScope-accredited installer, we deliver manufacturer-backed product warranties on eligible Colorbond installations.

Metal roofing is lightweight, durable, low-maintenance and available in a wide range of profiles and colours to suit everything from a heritage home in New Farm to a contemporary architect-designed house in Paddington or a coastal property in Burleigh Heads.

Profiles & Products

## The right profile for the application

### Corrugated (Classic Rib)

The iconic Australian corrugated profile in modern Colorbond — suited to heritage restorations, rural properties and contemporary homes.

### Trimdek & Custom Orb

Wider-rib profiles offering broader coverage per sheet, faster installation and a slightly more contemporary look.

### Longline / Hi-Ten

Extended rib height for improved structural performance under wind load — used on commercial and industrial buildings.

### Standing Seam / Concealed Fix

Hidden fasteners for a clean, uninterrupted roofline — popular on architect-designed homes and premium commercial builds.

### Klip-Lok & Snap-Lock

Factory-formed concealed-fix profiles with high wind-uplift resistance, widely used in SEQ’s higher wind classifications.

### Colorbond Coolmax

Reflects radiant heat to reduce summer cooling loads — in 22 standard and heritage colours from Surfmist to Basalt.

Wind Loads & Warranties

## Installed to your calculated wind classification

SEQ is classified primarily as Wind Region B under AS 4055, with coastal and exposed areas reaching Region C or higher. We calculate the classification for each project and specify fastening accordingly.

- Wind calculation per project based on location, terrain and building height.
- Compliant fastening — sheet-to-purlin connections meeting the calculated uplift forces.
- Certifier documentation provided where required for building certifiers.
- BlueScope product warranty on eligible Colorbond and Zincalume installs.
- Workmanship guarantee in addition to the manufacturer warranty.
- Coastal specification for salt-air environments from Redcliffe to the Gold Coast.

Common Questions

## Frequently asked questions

Surfmist and Monument remain consistently popular across Greater Brisbane. Coastal Gold Coast properties often favour Shale Grey and Windspray; heritage inner-city homes often opt for Paperbark or Basalt. We can provide samples for your specific project.

Metal roofing with appropriate sarking, insulation and ceiling systems is no noisier than tile in heavy rain. Sarking and insulation batts significantly reduce rain noise — we can advise on the right specification for your project.

Yes — concealed-fix and standing seam systems carry a premium due to materials and installation complexity. For architect-designed homes or premium commercial projects, the result is typically worth the investment.

A correctly installed Colorbond roof in SEQ will typically last 40 years or more. BlueScope’s product warranty for eligible installations covers perforation by corrosion for the warranted period.

Related Services

## Explore more roofing services

Domestic Roofing
Commercial Roofing
Architectural Cladding
Roof Replacement
Free, No-Obligation Quote

## Discuss your metal roofing project

From corrugated to concealed-fix — talk to a BlueScope-accredited installer.

Request a quote
Call 0488 773 232